Evaluating the effectiveness of wood shred and agricultural straw mulches as a treatment to reduce post-wildfire hillslope erosion in southern British Columbia, Canada, Robichaud, P. R., Jordan P., Lewis S. A., Ashmun L. E., Covert S. A., and Brown R. E. , Geomorphology., Volume 197, (2013)

Production and aerial application of wood shreds as a post-fire hillslope erosion mitigation treatment, Robichaud, Peter R., Ashmun Louise E., Foltz Randy B., Showers Charles G., J. Groenier Scott, Kesler Jennifer, DeLeo Claire, and Moore Mary , Number Gen. Tech. Rep. RMRS-GTR-307, Fort Collins, CO, (2013)

An analytical method for predicting postwildfire peak discharges, Moody, J.A. , U.S. Geological Survey Scientific Investigations Report, Number 2011-5236, (2012)

After the fire is out, LeQuire, E. , Fire Science Digest, Volume 10, (2011)

Modeling hydrologic and geomorphic hazards across post-fire landscapes using a self-organizing map approach, Friedel, M.J. , Environmental Modelling and Software, Volume 26, (2011)

The effectiveness of aerial hydromulch as a post-fire erosion control treatment in southern California, Wohlgemuth, P.M., Beyers J.L., and Robichaud P.R. , Proceedings of the Joint Federal Interagency Conference, 9th Federal Interagency Sedimentation Conference and 4th Federal Interagency Hydrologic Modeling Conference, Las Vegas, NV, (2010)

Synthesis of sediment yields after wildland fire in different rainfall regimes in the western United States, Moody, J. A., and Martin D. A. , International Journal of Wildland Fire, Volume 18, Issue 1, (2009)

Post-wildfire erosion response in two geologic terrains in the western USA, Moody, J. A., Martin D. A., and Cannon S.H. , Geomorphology, Volume 95, (2008)